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A CARRIER CANCELLATION SYSTEM 
Abstract
This document describes a carrier cancellation system that is configured to generate a cancellation signal having an amplitude and phase that is almost equal to the amplitude and phase of a received carrier signal thereby effectively cancelling the carrier signal. The system is able to achieve such a close match between the amplitudes and phases of the two signals through the use of an initialized logic control module that was pre-initialized using a dual iterative approach to select an optimal starting phase entry and an optimum gain entry which are then used to generate the cancellation signal.  
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