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540 Degree of access FAR-UVC light disinfection station with rotating base platform


Brief Description of the Drawings

[0001] FIG. 1 illustrates a concept of the design of the disinfection station, where a stationary arc shape frame is setup above the rotating base platform. 
[0002] Component #1 is the stationary frame, shape could be arc, rectangular, square etc, with height in the range of 2 to 3m, for mounting the FAR-UVC lights points.
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[0003] FIG. 1,2,3 illustrates the rotation of the base platform with an object on the platform with different angle.
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FIG 3
[0004] 
FIG. 4 illustrates 5 point of FA-UVC lights design of the disinfection station, on the stationary arc shape frame is setup above the rotating base platform6.FAR_UVC 
light#1
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