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ROTARY SPRAY JET CLEANING SYSTEM AND METHOD THEREFOR
ABSTRACT
		The present invention provides a cleaning system for a component having a center through hole, the cleaning system comprises a closable chamber having a cavity space therein for loading the component to be cleaned and a nozzle assembly having a nozzle tip that extended into the closable chamber to reach the center hole of the component.  The nozzle assembly is connected to an air source and a water source.  Operationally, the nozzle tip simultaneously provides spinning jet sprays to clean the component, wherein the spinning jet sprays comprises air spray and water spray in an alternate manner.  A method of cleaning the component is also provided. 
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