Attorney Docket No.: BALP2026NAT20WOSG0
ABSTRACT
Provided are a battery cover plate assembly and a power battery. The battery cover plate assembly includes a cover plate sheet (1), a conductive sheet (2) and a terminal (3). The cover plate sheet (1) is provided with a first connection hole (11). The conductive sheet (2) is provided with a second connection hole (21) and is mounted on an outer side of the cover plate sheet (1) and is configured to be welded to a current-conducting busbar (7). The terminal (3) has a first end folded outwards to form a first flange (31) and a second end provided with a connection wall (32). The connection wall (32) has a preset wall thickness. An inner side of the connection wall (32) is configured to be welded to a current collector (8), and an outer side edge of the connection wall (32) is provided with a second flange (33). After the second end of the terminal (3) is disposed to pass through the first connection hole (11) and the second connection hole (21) in sequence via an inner side of the cover plate sheet (1), the first flange (31) abuts against an inner wall of the cover plate sheet (1). The second flange (33) is folded outwards to rivet a side of the conductive sheet (2) away from the cover plate sheet (1).
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