ABSTRACT 
A FRUIT HARVESTING APPARATUS


The present invention discloses a fruit harvesting apparatus comprising an extraction timing detection device for automatically determining when to activate or deactivate a power source for cutting a fruit, the power source operably connected to the extraction timing detection device such that the power source is activated or deactivated based on the determination of the extraction timing detection device. The apparatus includes a controller in electrical communication with the extraction timing detection device and the power source, a support member operably attached to the extraction timing detection device at its end and a harvesting means in electrical communication with the power source for extracting the fruit.
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