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[bookmark: OLE_LINK78][bookmark: OLE_LINK89][bookmark: OLE_LINK10][bookmark: OLE_LINK11].ABSTRACT
[bookmark: OLE_LINK2][bookmark: OLE_LINK5][bookmark: OLE_LINK48][bookmark: OLE_LINK49]A cover assembly includes a bare aluminum sheet (1), a terminal (2), a pressing block (3), an upper plastic member (4) and a sealing member (5). The terminal (2) sequentially passes through a through hole in the bare aluminum sheet (1), a through hole in the upper plastic member (4) and a through hole in the pressing block (3). The upper plastic member (4) is sandwiched between the bare aluminum sheet (1) and the pressing block (3). The sealing member (5) is sleeved on the terminal (2), and the sealing member (5) includes a tubular portion (51). A cutting ring (511) is annularly arranged at a first end of the tubular portion (51) in an axial direction of the tubular portion (51), and the cutting ring (511) is arranged between the first end of the tubular portion (51) and the pressing block (3). The hardness of the cutting ring (511) is greater than the hardness of a rest structure of the tubular portion (51). The cutting ring (511) abuts against the pressing block (3). The tubular portion (51) is partially sandwiched between the terminal (2) and an inner wall of the through hole of the upper plastic member (4), and is partially sandwiched between the terminal (2) and an inner wall of the through hole of the bare aluminum sheet (1).
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