ABSTRACT
The present invention comprises a novel protective face shield consisting of at least one visor produced from transparent plastic sheet that encircles the face with a superior peripheral fit for improved protection of the wearer from harmful agents in the air. The air comes into the face shield from the top or bottom or sides of the shield and filters can be applied on these ventilation openings to filter the incoming air, thereby increasing the protection from airborne contaminants. The open edges of the face shield are covered with a seal for increased comfort to the wearer and elastic bands can be attached on the sides of the visor to support wearing it.
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