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Receive, at a certificate authority, a micro certificate signing
request from a computing device

Authenticate the micro certificate signing request

Generate a response to the micro certificate signing request

Verify the response to the micro certificate signing request

Transmit the response to the computing device, where a micro
certificate signed by the certificate authority is reconstructed
based on the response
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