
A design of surgical mask with elastic cord as nose-bridge


SUMMARY OF THE INVENTION

The invention is using ear loop folded on mask. ear loop [200] is typical elastic cord, adjustable loop or fixed loop. the ear loop [200] is folded on mask [101]. 
Ear loop [200] is attached to the mask [100] at center of mask as shown in fig 2. only 2 points of ear loop [200] is welded at center of mask [201]. The rest of ear loop is flexible inside folding line, which enable ear loop fastening when mask [100] hanged over ears through  ear loop.[200].
The structure of ear loop [200] is to prevent a gap btw mask and nose, this is ‘automatically’ secures the nose-bridge. This new nose-bridge is connected to the elastic cord so when the user puts the mask on, it will lock in.
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