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Figure 1 shows the sorting of large waste materials.
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Figure 2 shows the sorting of ferrous metals and non-ferrous metals.
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Figure 3 shows the sorting of thin film waste, low density or low weight plastics and other plastics.
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Figure 4 shows the detailed view of the conveyor tray in Figure 1, 2 and 3.
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Figure 5A shows the overview of the thin film waste and the low density or low weight plastics processing stage.
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Figure 5B shows the thin film waste and the low density or low weight plastics being compressed.
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Figure 5C shows the elongation stage of the hydraulic piston rod to compress the plastic input.
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Figure 5D shows the output of the plastic cubes extracted from the output door.
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Figure 6 shows a detailed view of elongation of the hydraulic piston rod to compress the plastic waste.
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Figure 7 shows the granulation chamber for plastic & thin film, paper, cardboard, and organic waste.  
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Figure 8 shows the acetogenic chamber.
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Figure 9 shows the cellulose based plastic extraction from solid and liquid accumulation.
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Figure 10 shows the cellulose based plastic extraction from gaseous accumulation.
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