
A design of surgical mask with elastic cord as nose-bridge

ABSTRACT	

The face mask includes a main part and a number of fastening cord, which is connected to two sides of the main part. The main part includes a non-woven fabric created using a melt blowing process. The blue (or green) side of the mask (the fluid-repellant layer) is to be worn outward, with the white (absorbent) layer on the inside. A ear loop is commonly used on face mask to fasten face mask on a personal face. there is ear loop on both side, which is attached to 3-layer structure. One ear loop at top of mask is folded in mask and welded at center to replace nose bridge, or as called nose wire. Ear loop act as a nose bridge, which enable self-fastening when it is hanged over ears.
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